Q.18.Create a directory and on directiory set permission in away that user ditiss and dac can read and

write but vlsi neither read or write.

